**REQUEST FOR QUOTATION**

**Supply and delivery of Semi-Expendable ICT Equipment for Human Resource Office of MinSU Main Campus**

 **PR No. PR22-0387**

 **RFQ No. 2022 -206**

**ABC Amount: Php 103,500.00**

Company Name : **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

Address : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Please quote your lowest price on the items / listed below, subject to the General Condition on the last page, stating the shortest time of delivery and submit your quotation duly signed by your representative not later than **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** in the address stated in the last page.

 **NEMESIO H. DAVALOS, Ph.D.**

 BAC Chairperson

**Note: 1. All entries must be typewritten.**

 **2. Delivery Period within \_\_\_ calendar days.**

 **3. Warranty shall be for a period of six (6) months for supplies and materials, one (1) year for Equipment, from date**

 **of acceptance by the procuring entity.**

 **4. Price validity shall be a period of 30 calendar days.**

 **5. G-EPS Registration Certificate shall be attached upon submission of the Quotation.**

 **6. Bidders shall submit Original Brochures showing certification of the product being offered (optional).**

 **7. Mode of delivery: [ ] Pick-up (Schedule) [ ] Door to Door Delivery**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Unit** | **ITEM AND DESCRIPTION** | **QTY.** | **UNIT PRICE** | **TOTAL AMOUNT** |
| 1 | units | **Uninterruptible Power Supply (UPS)** | 3 |  |  |
|  |  | *Model GH11-1KVA* |  |  |  |
|  |  | *INPUT Nominal Voltage 220/230/240Va* |  |  |  |
|  |  | *Voltage Range 110-300Vac (160-300 Vac at*  |  |  |  |
|  |  | *100% load;110-300Vac at 50% load)* |  |  |  |
|  |  | *Frequency range 50/60Hz (auto-sensing), 40-70Hz range* |  |  |  |
|  |  | *Power Factor 0.99* |  |  |  |
|  |  | *OUTPUT Nominal; Voltage 220/230/240Vac* |  |  |  |
|  |  | *Voltage Regulation +/- 1%* |  |  |  |
|  |  | *Frequency 50Hz or 60Hz +/-0.1 Hz* |  |  |  |
|  |  | *Transfer Time Zero* |  |  |  |
|  |  | *Output Socket 3x Universal Type (Surge Protection)* |  |  |  |
|  |  | *waveform Pure Sinewave* |  |  |  |
|  |  | *True double-conversion; microprocessor control optimizes reliability* |  |  |  |
|  |  | *Adjustable charging current via LCD or software (1A-6A) only available for 6K/10K models* |  |  |  |
|  |  | *Smart SNMP works well with either USB or RS-232 together* |  |  |  |
|  |  | *Comprehensive display allows easy monitoring and access of UPS Status* |  |  |  |
| 2 | units | **Automatic Voltage Regulator** | 3 |  |  |
|  |  | *PVS Voltage Stabilizer 3KVA/2400W* |  |  |  |
|  |  | *PVS 3001CD 3KVA Servo Motor* |  |  |  |
|  |  | *Controlled AVR with Digital Display* |  |  |  |
| **Xvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvx** |  |
|  | **TOTAL** |  |

 **After having carefully read and accepted your General Condition, I / We quote you on the item at prices noted above**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Supplier’s Signature over Printed Name

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 TIN No. of Establishment

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Contact Number

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Date