**REQUEST FOR QUOTATION**

**Supply and Delivery of ICT Equipment for Auxiliary Office at MinSU**

 **PR No. PR22-346**

 **RFQ No. 2022 -191**

**ABC Amount: Php 100,000.00**

Company Name : **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

Address : \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Please quote your lowest price on the items / listed below, subject to the General Condition on the last page, stating the shortest time of delivery and submit your quotation duly signed by your representative not later than **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** in the address stated in the last page.

 **NEMESIO H. DAVALOS, Ph.D.**

 BAC Chairperson

**Note: 1. All entries must be typewritten.**

 **2. Delivery Period within \_\_\_ calendar days.**

 **3. Warranty shall be for a period of six (6) months for supplies and materials, one (1) year for Equipment, from date**

 **of acceptance by the procuring entity.**

 **4. Price validity shall be a period of 30 calendar days.**

 **5. G-EPS Registration Certificate shall be attached upon submission of the Quotation.**

 **6. Bidders shall submit Original Brochures showing certification of the product being offered (optional).**

 **7. Mode of delivery: [ ] Pick-up (Schedule) [ ] Door to Door Delivery**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item No.** | **Unit** | **ITEM AND DESCRIPTION** | **QTY.** | **UNIT PRICE** | **TOTAL AMOUNT** |
| 1 | unit | Desktop Computer (Complete Set) | 1 |  |  |
|  |  | *Specification:* |  |  |  |
|  |  | *Processor:* |  |  |  |
|  |  | *AMD Ryzen 7 5800X* |  |  |  |
|  |  | *CPU Socket Type: Socket AM4* |  |  |  |
|  |  | *# of Cores: 8-Core* |  |  |  |
|  |  | *# of Thread: 16* |  |  |  |
|  |  | *Motherboard:* |  |  |  |
|  |  | *B550M* |  |  |  |
|  |  | *Socket: AMD Socket AM4* |  |  |  |
|  |  | *Chipset: AMD B550 Chipset* |  |  |  |
|  |  | *Memory:* |  |  |  |
|  |  | *DDR4* |  |  |  |
|  |  | *Form Factor: Micro ATX* |  |  |  |
|  |  | *Maximum Memory Supported: 128GB* |  |  |  |
|  |  | *32gb DDR4 Memory* |  |  |  |
|  |  | *Support Intel XMP 2.0 smart overclocking technology* |  |  |  |
|  |  | *Selected high quality IC chips* |  |  |  |
|  |  | *Module Type: 288 Pin Unbuffedered DIMM Non ECC* |  |  |  |
|  |  | *Frequency: 3200* |  |  |  |
|  |  | *PC Case* |  |  |  |
|  |  | *Support EATX, ATX, Micro ATX & Mini ATX Motherboard* |  |  |  |
|  |  | *Drive Bay : 2x HDD & 2x SSD* |  |  |  |
|  |  | *CPU height limit 160mm* |  |  |  |
|  |  | *Left Side Panel: Hinge Type Tempered Glass* |  |  |  |
|  |  | *Solid State Drive* |  |  |  |
|  |  | *Form Factor : 2.5"* |  |  |  |
|  |  | *NAND Flash: 3D QLC* |  |  |  |
|  |  | *240gb Solid State Drive* |  |  |  |
|  |  | *Power Supply* |  |  |  |
|  |  | *650 watts* |  |  |  |
|  |  | *PSU FORM FACTOR : ATX* |  |  |  |
|  |  | *INPUT FREQUENCY: 50Hz - 60Hz* |  |  |  |
|  |  | *INPUT VOLTAGE: 100-240Vac* |  |  |  |
|  |  | *Videocard* |  |  |  |
|  |  | *RTX 3060* |  |  |  |
|  |  | *CUDA cores: 3584* |  |  |  |
|  |  | *Video Memory: 12GB GDDR6* |  |  |  |
|  |  | *Memory Bus: 192-bit* |  |  |  |
|  |  | *Display ports: 3DP + HDMI* |  |  |  |
|  |  | *Core Clock: Base: 1320Mhz; Boost: 1777Mhz* |  |  |  |
|  |  | *Monitor:* |  |  |  |
|  |  | *Panel Size: Wide Screen 23.8" (60.5cm) 16:9* |  |  |  |
|  |  | *Color Saturation: 72% NTSC* |  |  |  |
|  |  | *Panel Type: IPS* |  |  |  |
|  |  | *True Resolution: 1920x1080* |  |  |  |
|  |  | *Display Viewing Area (HxV): 527.04 x 296.46 mm* |  |  |  |
|  |  | *Display Surface: Non-glare* |  |  |  |
|  |  | *Pixel Pitch: 0.2745 mm* |  |  |  |
|  |  | *Brightness: 250 cd (Typical)* |  |  |  |
|  |  | *Contrast Ratio 1000: 1 (Typical)* |  |  |  |
|  |  | *ASUS Smart Contrast Ratio (ASCR): 100000000 : 1* |  |  |  |
|  |  | *Viewing Angle (CR?10): 178 (H) /178(V)* |  |  |  |
|  |  | *Response Time: 1ms MPRT, 4ms (Gray to Gray)* |  |  |  |
|  |  | *Display Colors: 16.7M* |  |  |  |
|  |  | *Flicker Free: Yes* |  |  |  |
|  |  | *Refresh Rate (max): 144Hz* |  |  |  |
|  |  | *Video Feature* |  |  |  |
|  |  | *trace Free Technology : Yes* |  |  |  |
|  |  | *SPLENDID Video Preset Modes: 8 Modes (sRGB Mode/ Scenery Mode/ Theater Mode/ Standard Mode/ Night View)* |  |  |  |
|  |  | *Mode/ Game Mode/ Reading Mode/ Darkrom Mode)* |  |  |  |
|  |  | *Skin-Tone Selection: 3 Modes* |  |  |  |
|  |  | *Color Temperature Selection: 4 Modes* |  |  |  |
|  |  | *Quick Fit (modes): Yes (Alignment Grid/ Paper/ Photo Modes)* |  |  |  |
|  |  | *GamePlus (modes): Yes (Crosshair/ Timer/ FPS Counter/ Display Alignment)* |  |  |  |
|  |  | *Low blue Light: Yes* |  |  |  |
|  |  | *HDCP support: Yes* |  |  |  |
|  |  | *FreeSync technology supported* |  |  |  |
|  |  | *Adaptive-Sync supported: Yes* |  |  |  |
|  |  | *Extreme Low Motion Blur* |  |  |  |
|  |  | *Shadow Boost* |  |  |  |
|  |  | *Audio Features* |  |  |  |
|  |  | *Stereo Speakers: 2W x 2 Stereo RMS* |  |  |  |
|  |  | *I/O Ports* |  |  |  |
|  |  | *Signal Input: HDMI, D-Sub, Displayport* |  |  |  |
|  |  | *PC Audio Input: 3.5mm Mini-Jack* |  |  |  |
|  |  | *Signal Frequency* |  |  |  |
|  |  | *Analog Signal Frequency: 30-84KHz (H)/48 -75 Hz(V)* |  |  |  |
|  |  | *Digital Signal Frequency: 30-180 KHz(H) / 48-144 Hz(V)* |  |  |  |
|  |  | *Power Consumption* |  |  |  |
|  |  | *Power On 9Typical):< 16W\** |  |  |  |
|  |  | *Power Saving Mode: <0.5W* |  |  |  |
|  |  | *Power Off Mode: <0.5W* |  |  |  |
|  |  | *Voltage: 100-240V, 50/60Hz* |  |  |  |
|  |  | *Mechanical Design* |  |  |  |
|  |  | *Chassis Colors: Black* |  |  |  |
|  |  | *Tilt: +20-5* |  |  |  |
|  |  | *VESA Wall Mounting: 100x100mm* |  |  |  |
|  |  | *Frameless Design: Yes* |  |  |  |
|  |  | *Security* |  |  |  |
|  |  | *Kensington lock* |  |  |  |
|  |  | *Dimensions* |  |  |  |
|  |  | *Dimension with Stand (WxHxD): 540.50 x 389.34 x 204.42 mm* |  |  |  |
|  |  | *Dimension without Stand (WxHxD) 540.50 x 325.24 x 51.67mm* |  |  |  |
|  |  | *Box Dimension (WxHxD): 599 x 446 x 136mm* |  |  |  |
|  |  | *Weight* |  |  |  |
|  |  | *Net Weight 9Esti): 3.56 kg* |  |  |  |
|  |  | *Net Weight without Stand (For VESA Wall mount) (Esti): 3.07 kg* |  |  |  |
|  |  | *Gross Weight (Esti): 5.8kg* |  |  |  |
|  |  | *Accessories* |  |  |  |
|  |  | *VGA Cable (Optional)* |  |  |  |
|  |  | *Audio Cable (Optional)]\Power Cord* |  |  |  |
|  |  | *Display Port cable (Optional)* |  |  |  |
|  |  | *Quick Start guide* |  |  |  |
|  |  | *HDMI cable (Optional)* |  |  |  |
|  |  | *Model: UPS - 3000VA* |  |  |  |
|  |  | *Input Voltage: 220/230/240V 1 Phase 50 Hz/60Hz + Hz* |  |  |  |
|  |  | *Output Socket: 6 (5 UPS + 1BYPASS)* |  |  |  |
|  |  | *Transfer Time: Typical 2-6ms* |  |  |  |
|  |  | *Waveform (Batt. Mode) Stimulated Sine wave* |  |  |  |
|  |  | *Dimension D x W x H (mm): L406x H245mm* |  |  |  |
|  |  | *BATTERY type: Sealed , maintenance - free lead acid* |  |  |  |
|  |  | *Typical recharge Time: 9-10 hours* |  |  |  |
|  |  | *Protection: Automatic self-test & discharge protection, replace battery indicator* |  |  |  |
|  |  | *Backup Time 6-30 minutes(depending on computer load)* |  |  |  |
|  |  | *Inverter compatible* |  |  |  |
|  |  | *Excellent microprocessor Control* |  |  |  |
|  |  | *Guarantees High Reliability* |  |  |  |
|  |  | *boost and Buck AVR for voltage stabilization* |  |  |  |
|  |  | *Off-mode charging* |  |  |  |
|  |  | *Cold start function* |  |  |  |
|  |  | *with keyboard and mouse* |  |  |  |
| **Xvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvxvx** |  |
|  | **TOTAL** |  |

 **After having carefully read and accepted your General Condition, I / We quote you on the item at prices noted above**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Supplier’s Signature over Printed Name

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 TIN No. of Establishment

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Contact Number

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Date

**General Conditions**

1. Quotations and other requirements stated below shall be submitted to the **Bids and Awards Committee (BAC) Office, Mindoro State University -Main Campus, Alcate, Victoria, Oriental Mindoro**, Philippines on the date and time stated in this RFP.
2. Supplier shall submit the following requirements:
3. Duly signed original copy of Request for Quotation (RFQ). Prices shall be quoted in Philippine Pesos.
4. PhilGEPS Registration
5. Valid Mayor’s/Business Permit
6. Omnibus Sworn Statement
7. BIR Certificate of Registration
8. Latest Income/Business Tax Return
9. TAX Clearance
10. DTI Registration/SEC Certificate
11. Original Brochures or certificates of the items offered showing its performance characteristics or specifications, if applicable

**Price validity shall be 30 calendar days from the deadline of submission of quotation.**

**Ocular Inspection**

Upon the decision of the End-User and BAC, the supplier and its concerned premises may be subjected to ocular inspection and approval by the End-User and/or TWG Inspections of the BAC prior to the award.

**Award**

The supplier that submitted the lowest calculated responsive quotation, and passed the inspection conducted by the End-User and BAC prior to the event, if any, shall be awarded the contract.

**Evaluation of Quotations**

Quotations shall be compared and evaluated of the basis of the following criteria:

1. Completeness of Submission
2. Compliance with Item & Description Requirements
3. Price

**Instructions**

1. Supplier shall be responsible for the source(s) of its goods/services/equipment, and which shall be in accordance with the schedule and specifications of the RFQ or contract. Failure of the supplier to comply with this provision shall be ground for cancellation of the award or purchase order issued to the supplier.
2. Supplier that accepted an award, purchase order, or contract but failed to deliver the required goods/services/equipment within the time called for in the award, purchase order, or contract shall be disqualified from participating in MinSU or any of MinSU campuses future procurement activities. This is without prejudice to the imposition of other sanctions prescribed under R.A. 9184 and its IRR-A against the supplier.
3. All duties, excise, and other taxes and revenue charges shall be paid by the supplier.
4. All transactions are subject to withholding of credible Government Taxes per revenue regulation(s) of the Bureau of Internal Revenue

**Liquidation Damages**

A penalty of one-tenth of one percent (0.001) of the total value of the undelivered goods/services/equipment shall be charged as liquidated damages for every day of delay of the delivery of the purchased goods/services/equipment.

**Warranty**

Supplier warrants that all goods/services/equipment to be provided are of acceptable industry standard.

**Payment**

Payment shall be made only upon a certification by the Head of the Procuring Entity to the effect that the GOODS have been rendered or delivered in accordance with the terms of this Contract and have been duly inspected and accepted.